Aguas, H, Pereira, L, and Raniero. "{MIS photodiodes of polyrnorphous silicon deposited at higher growth rates by 27.12 MHz PECVD discharge}." 455-456 (2004): 73-76.